REACTOR SIZING

By using CSTR

, since for CSTR no accumulation occur over time.

Assuming

* First order reaction
* Conversion at optimum yield = 0.35

Based on the data collected, FA0 of crude oil produced = input = 34.6 kg/day

Where,

By rounding off to the nearest liter,